From Bu:

3. K. Ofuchi and D. Kunii, Heat-Transfer Characteristics of Packed Beds with Stagnant Fluids, Int. J. Heat. Mass. Transfer, vol. 8, pp. 749–757, 1965.

4. M. M. Yovanovich, Thermal Contact Resistance across Elastically Deformed Spheres, J. Spacecraft., vol. 4, pp. 119–122, 1967.

~~5. G. K. Batchelor and R. W. O’Brien, Thermal or Electrical Conduction Through a Granular Material, Proc. R. Soc. London A., vol. 355, pp. 313–333, 1977.~~

6. S. Hayashi, K. Kubota, H. Masaki, Y. Shibata, and K. Takahashi, A Theoretical Model For The Estimation of the Effective Thermal Conductivity of a Packed Bed of Fine Particles, Chem. Eng. J., vol. 35, pp. 51–61, 1987.

7. J. Sun and M. M. Chen, A Theory Analysis of Heat Transfer due to Particle Impact, Int. J. Heat. Mass. Transfer, vol. 31, pp. 969–975, 1988.

8. C. Aargento and D. Bouvard, Modeling the Effective Thermal Conductivity of Random Packing of Spheres through Densification, Int. J. Heat. Mass. Transfer,vol.39, pp. 1343–1350, 1996.

9. C. Mihalyko, B. G. Lakatos, and T. Blickle, Modeling Heat Transfer between Solid Particles, Comput. Simulat., vol. 53, pp. 403–408, 2000.

Population balance models for colliding spheres

10. M. Bahrami, M. M. Yovanovich, and J. R. Culham, Thermal Contact Resistance of Nonconforming Rough Surface, Part 2: Thermal Model, J. Thermophys. Heat. Transfer, vol. 18, pp. 218–227, 2004.

They create an effective conductivity. Use this for validating CFD-DEM for stagnant fluid